digital_input group

This group contains all digital input signals.

Each signal is a sub group with the signal name as the group name.

pad

defines the chip pad that the signal should be read from.

type: string