command C

Format: ‘C sig[;addr]’

Meaning: Continue with signal sig (hex signal number). If ‘;addr’ is omitted, resume at same address.

This packet is deprecated for multi-threading support. Use vCont command.