command D

Format: ‘D[;pid]’

Meaning: Without pid this detaches from the target MCU. With pid given (multiprocess protocol extension) it detaches from the given process. pid is a big-endian hex string.

Reply:

OK