STM32F429

ARM Cortex-M4 (180MHz) FPU

Memory Map

start address	end address	used for	comment
0x0	0x1fffff	Aliased to flash, system memory or SRAM depending on the BOOT pins
0x20 0000	0x7ff ffff	reserved
0x800 0000	0x81f ffff	flash memory
0x820 0000	0xfff ffff	reserved
0x1000 0000	0x1000 ffff	CCM data RAM	64 KB SRAM
0x1001 0000	0x1ffe bfff	reserved

Peripherals

IRQ

IRQ Number	Signal

Clocks

UART

GPIO

Function select

Nucleo-F429ZI board

abbreviation dictionary

abbreviation	long version	comment