command c

Format: ‘c [addr]’

Meaning: Continue at addr, which is the address to resume. If addr is omitted, resume at current address.

This packet is deprecated for multi-threading support. Use vCont command.