command qIsAddressTagged

Format: ‘qIsAddressTagged:address’

Meaning: Check if address address is in a memory tagged region; if it is, it’s said to be tagged. The target is responsible for checking it, as this is architecture-specific.

address is the address to be checked.

Reply: Replies to this packet should all be in two hex digit format, as follows:

01

Address address is tagged.

00

Address address is not tagged.