command QNonStop

Format: ‘QNonStop:x’

Meaning: Enter non-stop (‘QNonStop:1’) or all-stop (‘QNonStop:0’) mode. This packet is not probed by default; the remote stub must request it, by supplying an appropriate ‘qSupported’ response.

Reply:

OK